# Laser GUI Help and Documentation

## How to start

1. **Double click laserGUI.bat in “Laser” file.** A command prompt will appear, followed by the Laser Control GUI shortly after.
2. **DONE!** You’ve successfully opened the GUI.

## Step 1: Alignment

Sections [Left alignment point] and [Right alignment point]

1. Put your wafer into the laser.
2. Open the 3DMM Laser control program at the laser’s PC.
3. Go to the corresponding laser positions using the jog sheet

## Step 2: rasterfahrt

TroubleShoot

ValueError: could not convert string to float:

Most probably empty column